This is the Intel(R) RSTe 4.5 F6 installation and driver zip files for PV Version Package 4.5.0.1335.
The contents of this zip file include the F6 installation drivers and the standard OS drivers to
support manual driver installation activities.  The following are the directories and their 
contents included in RSTe_4.5.0.1335_F6-drivers.zip:

iaStorA.free.win7.32bit.4.5.0.1234   – The 32 bit ACHI drivers for Windows 7.
iaStorA.free.win7.64bit.4.5.0.1234   – The 64 bit ACHI drivers for Windows 7 and Windows Server
                                       2008 R2.
iaStorA.free.win8.32bit.4.5.0.1234   – The 32bit AHCI drivers for Windows 8.1/10/Server 2012/
                                       Server 2012 R2.
iaStorA.free.win8.64bit.4.5.0.1234   – The 64 bit AHCI drivers for Windows 8.1/10/Server 2012/
                                       Server 2012 R2.
iaStorS.free.win7.32bit.4.5.0.1234   – The 32 bit SCU driver for Windows 7.
iaStorS.free.win7.64bit.4.5.0.1234   – The 64 bit SCU driver for Windows 7 and Windows Server 
                                       2008 R2.
iaStorS.free.win8.32bit.4.5.0.1234   – The 32bit SCU driver for Windows 8.1/10/Server 2012/
                                       Server 2012 R2.
iaStorS.free.win8.64bit.4.5.0.1234   – The 64bit SCU driver for Windows 8.1/10/Server 2012/
                                       Server 2012 R2.

The same driver version applies to the drivers for manual installation.

For further questoins, please contact you Intel FAE.
